**LIST OF APPROVED BRANDS / MAKES INTERIOR & FURNISHING**

The Interior Works Subject To Approval of Samples by the Consultants / KSSFCL

All the Materials Used Have to Confirm To Green Interior Norms of IGBC

|  |  |  |
| --- | --- | --- |
| **Sl No** | **LIST OF MAKE** | **BRAND / MANUFACTURER** |
| 1 | PLYWOOD  | Century ply/ Greenply/Merino/Ambi Ply or Equivalent |
| 2 | FLEXIBLE PLYWOOD  | Century ply/ Greenply/Merino/Ambi Ply or Equivalent |
| 3 | LAMINATE  | Merino/Archid/Century ply/ Greenply or approved FSC equivalent |
| 4 | FLUSH DOORS | Century ply/Ambi Ply Greenply or approved FSC equivalent |
| 5 | VENEER  | Century ply/ Greenply/Merino or Equivalent |
| 6 | LOCKS | Dorma/Dorset/D-line/ IR/ Hager/ Hafele/ Union/ Hettich/ Blum or Approved Equivalent |
| 7 | DOOR CLOSURE/ FLOOR SPRINGS  | Dorma /Ozone/Dorset/ D-line/ Union/ Hafele/ / or Approved Equivalent |
| 8 | HANDLES  | Ozone/Godrej/Doorset/Assaalbay or Equivalent |
| 9 | HINGES | Ozon/ Dorma/ IR/ Union/ Hager /Hafele/Hettich/Blum or Approved Equivalent |
| 10 | PROPRIETARY SLIDDING/ FOLDING DOORS | Ozone/Dorma or approved equivalent |
| 11 | PATCH FITTINGS  | Ozone/Dorma/ Union or Approved Equivalent |
| 12 | GLASS / MIRROR | Saint Gobain/ Modi float / Ashai or Approved Equivalent  |
| 13 | SCREWS | Nettle fold make / Equivalent confirming to IS 1365 |
| 14 | ALUMINIUM SECTIONS | Jindal/Bhoruka/Hindalco  |
| 15 | ALUMINIUM CLEATS (3mm) | Jindal/ Bhoruka/ Hindalco  |
| 16 | GRANITE\MARBLE SLABS | First Quality, Water-cut type of or Approved Equivalent |
| 17 | ITALIAN MARBLE SLABS | First Quality, Resin bonded, Imported or Approved Equivalent |
| 18 | ETCHING, FROSTING FILM/ VINYL SHEETS | 3M or Approved Equivalent |
| 19 | DIGITAL PRINTED VINYL | 3M or Approved Equivalent |
| 20 | EMULSION// LUSTER/ ENAMEL PAINTS/ |  Berger/ Nerolac/ Asian/ J & N/Jotun/ICI or Approved Equivalent |
| 21 | PRIMER | Berger/ Nerolac/ Asian/ J & N/Jotun/ICI or Approved Equivalent |
| 22 | PUTTY FOR PAINT | Asian / Birla Wall Putty, Epoxy, Thin coating Putty or Approved Equivalent |
| 23 | VINYL/ ANTI-STATIC FLOOR | Amstrong/ Gerflor/Tarkett/Forbo or Approved Equivalent |

|  |  |  |
| --- | --- | --- |
| **Sl No** | **LIST OF MAKE** | **BRAND / MANUFACTURER** |
| 24 | RUBBERISED VINYL FLOOR  | Amstrong/ Gerflor/Tarkett/Forbo or Approved Equivalent |
| 25 | OFFICE SEATINGS | Godrej / Featherlite / Eurosit or Equivalent |
| 26 | CORIAN HARD SURFACE | Merino Hanex / LG / or Equivalent |
| 27 | WRITING BOARD | White Mark Boards |
| 28 | ADHESIVES | Fevicol SH or Approved Equivalent |
| 29 | SLIDING CHANNELS | Hager/ Hettich/ Hafele or Approved Equivalent |
| 30 | POWDER COATING PAINT | MRF/ Marpol/ Berger  |
| 31 | GRG, PLAIN GYPSUM BOARD, SUSPENSION | India Gypsum Ltd/Gyproc |
| 32 | UNIVERSAL GYP PLASTER  | India Gypsum Ltd/Gyproc |
| 33 | PVC SPACERS/ CORNER BEADINGS | Arpitha Exports/ BOSS/Johnsonite or equivalent |
| 34 | GRG/ MR Grade/ GYPSUM BOARD WITH SUSPENSION SYM | India Gypsum Ltd/Gyproc |
| 35 | CALCIUM SILICATE BOARD WITH SUSPENSION SYM | Hilux - Ramco Industries Ltd  |
| 36 | FALSE CEILING SUSPENSION SYSTEM | India Gypsum Ltd/Gyproc/ AMSTRONG |
| 37 | UNIVERSAL GYP PLASTER (PUNNING)  | India Gypsum Ltd/Gyproc |
| 38 | STAINLESS STEEL SINK | AMC/ Nirali or Equivalent |
| 39 | CERAMIC TILES |  Kajaria World/ H& R Johnson/ Somany/Nitco |
| 40 | VITRIFIED TILES |  Johnson/ Nitco/ Bell/ Euro/Kajaria/Somany |
| 41 | SELF-LEVELLING COMPOUND FOR FLOOR | Roffee/ Fosroc or approved equivalent |
| 42 | POLYMER BASED CEMENTITOUS GROUTS | Laticrete/ Bal Endura or approved equivalent |
| 43 | FIRE RATED DOORS | Signum/ Promat or approved equivalent |
| 44 | STEEL FIRE RATED DOORS | Signum/ Shakti-Met-Dor or approved equivalent |
| 45 | PLASTER MESH | Arpitha Exports or Approved Equivalent |
| 46 | WHITE CEMENT | Birla White/ JK or approved equivalent |
| 47 | IMPORTED VITRIFIED TILES | Euro/ RAK or Approved Equivalent |